Berikut setingan game PB

Point Blank Online game

Masuk ke IP > firewall > mangle

chain=prerouting action=mark-connection new-connection-mark=pb.iix.a   
passthrough=yes protocol=udp dst-address=203.89.146.0/23   
dst-port=40000-40010   
  
1 chain=prerouting action=mark-packet new-packet-mark=pb.iix.p   
passthrough=no connection-mark=pb.iix.a   
  
2 ;;; PB IIX  
chain=prerouting action=mark-connection new-connection-mark=pb.iix.b   
passthrough=yes protocol=tcp dst-address=203.89.146.0/23   
dst-port=39100,39110,39220,39190,49100   
  
3 chain=prerouting action=mark-packet new-packet-mark=pb.iix.p   
passthrough=no connection-mark=pb.iix.b

masuk ke QUEUE TREE

0 name="PB" parent=lan packet-mark=pb.iix.p limit-at=1M queue=default   
priority=7 max-limit=3M burst-limit=0 burst-threshold=0 burst-time=0s

Untuk game lain silahkan anda masukan sendiri no port tcp/updnya tidak perlu dst-address